// Параметры ниже для удобства коммутации шлейфами с разным количеством контактов.
// [KB_pins=] кол-во контактов разъёма под клавиатуру (24/25/26/28/30/32/34)
// LEFT или RIGHT. Если при установке шлейфа от себя в разъём, первый контакт слева, то LEFT. В другом случае-RIGHT. 
// UP или DOWN - Контакты в разъеме клавиатуры находятся вверху или внизу. 
// 05MM/08MM/1MM   шаг между выводами в разьеме клавиатуры

// Parameters are below for convenience of switching by FFC with different number of contacts.
// [KB_pins =] number of pins for the keyboard connector (24/25/26/28/30/32/34)
// LEFT or RIGHT. If you install the FFC from yourself into the connector, the first contact on the left, then LEFT. In another case, RIGHT.
// UP or DOWN - Contacts in the keyboard connector are at the up or down.
// 05MM or 08MM or 1MM   contact pitch keyboard connector 
// FLASH= size flash EC (KB) Default-128KB
// ----------------------------------------------------------------------------------------------------------------------------------------------------------------------------
// In this list, MB is different from the standard. 
// Standart is KB_pins=30 JENK=7 TCK=19 TMS=20 TDI=21 TDO=10
// For reference about the EC contact numbers:  NPCE288N/388N pin number  ->  JENK=39   TCK=51   TMS=52   TDI=53   TDO=44        (SS)
//                                              NPCE288GA0DX  pin number  ->  JENK=53   TCK=52   TMS=51   TDI=50   TDO=48        (evserv)
//                                              NPCE388PB0BX  pin number  ->  JENK=D10  TCK=E13  TMS=E12  TDI=E10  TDO=F12       (evserv)
// ----------------------------------------------------------------------------------------------------------------------------------------------------------------------------

STANDART_1pin_LEFT   KB_pins=30 1MM LEFT  DOWN  JENK=7 TCK=19 TMS=20 TDI=21 TDO=10
STANDART_1pin_RIGHT  KB_pins=30 1MM RIGHT DOWN  JENK=7 TCK=19 TMS=20 TDI=21 TDO=10

LAR-1     KB_pins=36 LEFT DOWN 05MM FLASH=256 JENK=13 TCK=7 TMS=18 TDI=22 TDO=4    (evserv)  CHIP=NPCE288GA0DX
LAR-2     KB_pins=36 LEFT DOWN 05MM FLASH=384 JENK=7 TCK=13 TMS=11 TDI=14 TDO=17   (evserv)  CHIP=NPCE68BPA1DX

LBB-1     KB_pins=32 LEFT DOWN 05MM FLASH=256 JENK=13 TCK=7 TMS=18 TDI=22 TDO=4    (tested kinoxa)
LBB-2     KB_pins=32 LEFT DOWN 05MM FLASH=256 JENK=13 TCK=7 TMS=18 TDI=22 TDO=4    CHIP=NPCE388PB0BX (Pityu) TESTED_OK
LC56-14T  KB_pins=34 LEFT DOWN 08MM FLASH=256 JENK=20 TCK=16 TMS=14 TDI=9 TDO=17   CHIP=NPCE388PB0DX (Bilal)
LKL-1     KB_pins=40 LEFT DOWN 05MM FLASH=256 JENK=13 TCK=7 TMS=18 TDI=22 TDO=4    (evserv)
LKL-2     KB_pins=40 LEFT DOWN 05MM FLASH=256 JENK=13 TCK=7 TMS=18 TDI=22 TDO=4    (evserv) 
LLA-1     KB_pins=32 LEFT DOWN 05MM FLASH=256 JENK=7 TCK=13 TMS=11 TDI=14 TDO=17   (evserv)
LCL-1     KB_pins=32 LEFT DOWN 05MM FLASH=256 JENK=11 TCK=7 TMS=24 TDI=23 TDO=21   (evserv)
Mel_8L    KB_pins=40 LEFT DOWN 05MM FLASH=256 JENK=7 TCK=11 TMS=13 TDI=18 TDO=10   CHIP=NPCE38APB1DX (Piglet)

LA-B091P  (JKB1) KB_pins=26 LEFT 1MM    JENK=7   TCK=19 TMS=20 TDI=21 TDO=10
LA-B092P  (JKB1) KB_pins=26 LEFT 1MM    JENK=7   TCK=19 TMS=20 TDI=21 TDO=10
LA-B102P  KB_pins=26 LEFT               JENK=7   TCK=19 TMS=20 TDI=21 TDO=10
LA-B921P  KB_pins=26 LEFT               JENK=26 TCK=14 TMS=13 TDI=12 TDO=21
LA-C251P  KB_pins=26 LEFT               JENK=1 TCK=13 TMS=14 TDI=15 TDO=6       
LA-C311P  KB_pins=26 LEFT               JENK=7 TCK=19 TMS=20 TDI=21 TDO=10
LA-D061P  KB_pins=26 LEFT DOWN 08MM     JENK=7 TCK=19 TMS=20 TDI=21 TDO=10
LA-D102P  KB_pins=26 LEFT LEFT DOWN 1MM JENK=7   TCK=19 TMS=20 TDI=21 TDO=10
LA-D131P  KB_pins=26 LEFT               JENK=26 TCK=14 TMS=13 TDI=12 TDO=21
LA-C421P  KB_pins=32 LEFT DOWN 05MM     JENK=7 TCK=19 TMS=20 TDI=21 TDO=10
LA-D451P  KB_pins=32 LEFT               JENK=20 TCK=8 TMS=7 TDI=6 TDO=17
LA-D541P  KB_pins=32 LEFT               JENK=20 TCK=8 TMS=7 TDI=6 TDO=17
LA-D562P  KB_pins=32 LEFT DOWN 08MM     JENK=20 TCK=8 TMS=7 TDI=6 TDO=17
LA-E221P  KB_pins=32 LEFT DOWN          JENK=20 TCK=8 TMS=7 TDI=6 TDO=17
LA-E451P (JKB1) KB_pins=32 LEFT 08MM    JENK=20 TCK=8 TMS=7 TDI=6 TDO=17
LA-E581P  KB_pins=30 LEFT DOWN 08MM     JENK=20 TCK=8 TMS=7 TDI=6 TDO=17

NM-D391   KB_pins=40 LEFT DOWN 05MM FLASH=384 JENK=7 TCK=13 TMS=11 TDI=14 TDO=17 CHIP=NPCE68BPA0DX 0x0FE2201F (Дима_MD)
NM-C741   KB_pins=40 LEFT DOWN 05MM FLASH=256 JENK=7 TCK=13 TMS=11 TDI=14 TDO=17 CHIP=NPCE68APA0DX 0x0FE2201F (evserv)  
NM-C631   KB_pins=40 LEFT DOWN 05MM FLASH=256 JENK=7 TCK=13 TMS=11 TDI=14 TDO=17 CHIP=NPCE68APA0DX 0x0FE2201F (evserv)  


// Listed below are not currently supported EC! 
// NM-C262   KB_pins=40 LEFT DOWN 05MM FLASH=256 JENK=7 TCK=13 TMS=11 TDI=14 TDO=17   (evserv)  NPCX897KA0BX 0x4BA00477
// NM-C651   KB_pins=40 LEFT DOWN 05MM FLASH=256 JENK=7 TCK=13 TMS=11 TDI=14 TDO=17   (evserv)  NPCX897KA0BX 0x4BA00477
