
// Parameters are below for convenience of switching by FFC with different number of contacts.
// [KB_pins =] number of pins for the keyboard connector (24/25/26/28/30/32/34)
// LEFT or RIGHT. If you install the FFC from yourself into the connector, the first contact on the left, then LEFT. In another case, RIGHT.
// UP or DOWN - Contacts in the keyboard connector are at the up or down.
// 05MM or 08MM or 1MM   contact pitch keyboard connector 
// FLASH= size flash EC (KB) Default-128KB
// ----------------------------------------------------------------------------------------------------------------------------------------------------------------------------
// In this list, MB is different from the standard. 
// Standart is KB_pins=30 JENK=7 TCK=19 TMS=20 TDI=21 TDO=10
// For reference about the EC contact numbers:  NPCE288N/388N pin number  ->  JENK=39   TCK=51   TMS=52   TDI=53   TDO=44        (SS)
//                                              NPCE288GA0DX  pin number  ->  JENK=53   TCK=52   TMS=51   TDI=50   TDO=48        (evserv)
//                                              NPCE388PB0BX  pin number  ->  JENK=D10  TCK=E13  TMS=E12  TDI=E10  TDO=F12       (evserv)
// ----------------------------------------------------------------------------------------------------------------------------------------------------------------------------

STANDART_1pin_LEFT    KB_pins=30 1MM LEFT   DOWN  JENK=7 TCK=19 TMS=20 TDI=21 TDO=10
STANDART_1pin_RIGHT  KB_pins=30 1MM RIGHT DOWN  JENK=7 TCK=19 TMS=20 TDI=21 TDO=10
STANDART_1pin_ FLASH=256kb  KB_pins=30 1MM LEFT   DOWN  JENK=7 TCK=19 TMS=20 TDI=21 TDO=10

LBB-1     KB_pins=32 LEFT DOWN 05MM FLASH=256 JENK=13 TCK=7 TMS=18 TDI=22 TDO=4 (tested kinoxa)
LKL-1     KB_pins=40 LEFT DOWN 05MM FLASH=256 JENK=13 TCK=7 TMS=18 TDI=22 TDO=4    (evserv)
LKL-2     KB_pins=40 LEFT DOWN 05MM FLASH=256 JENK=13 TCK=7 TMS=18 TDI=22 TDO=4    (evserv) 
LLA-1     KB_pins=32 LEFT DOWN 05MM FLASH=256 JENK=7 TCK=13 TMS=11 TDI=14 TDO=17   (evserv)
LCL-1     KB_pins=32 LEFT DOWN 05MM FLASH=256 JENK=11 TCK=7 TMS=24 TDI=23 TDO=21   (evserv)

LA-B091P  (JKB1) KB_pins=26 LEFT 1MM JENK=7   TCK=19 TMS=20 TDI=21 TDO=10
LA-B092P  (JKB1) KB_pins=26 LEFT 1MM JENK=7   TCK=19 TMS=20 TDI=21 TDO=10
LA-B102P  KB_pins=26 LEFT JENK=7   TCK=19 TMS=20 TDI=21 TDO=10
LA-B921P  KB_pins=26 LEFT JENK=26 TCK=14 TMS=13 TDI=12 TDO=21
LA-C251P  KB_pins=26 LEFT JENK=1 TCK=13 TMS=14 TDI=15 TDO=6       
LA-C311P  KB_pins=26 LEFT JENK=7 TCK=19 TMS=20 TDI=21 TDO=10
LA-D061P  KB_pins=26 LEFT DOWN 08MM JENK=7 TCK=19 TMS=20 TDI=21 TDO=10
LA-D131P  KB_pins=26 LEFT JENK=26 TCK=14 TMS=13 TDI=12 TDO=21
LA-C421P  KB_pins=32 LEFT DOWN 05MM JENK=7 TCK=19 TMS=20 TDI=21 TDO=10
LA-D102p A-9 B-24 C-13 D-26 E-25
LA-D451P  KB_pins=32 LEFT JENK=20 TCK=8 TMS=7 TDI=6 TDO=17
LA-D541P  KB_pins=32 LEFT JENK=20 TCK=8 TMS=7 TDI=6 TDO=17
LA-D562P  KB_pins=32 LEFT DOWN 08MM JENK=20 TCK=8 TMS=7 TDI=6 TDO=17
LA-E221P  KB_pins=32 LEFT DOWN JENK=20 TCK=8 TMS=7 TDI=6 TDO=17
LA-E451P (JKB1) KB_pins=32 LEFT 08MM JENK=20 TCK=8 TMS=7 TDI=6 TDO=17
LA-E581P  KB_pins=30 LEFT DOWN 08MM JENK=20 TCK=8 TMS=7 TDI=6 TDO=17
LA-F971P REV 1.0 A20 B8 C17 D6 E7

nuvoton 288 and 388 technical data


SIGNAL HEADER  KEYBOARD  IO PIN 
-----------------------——————————
JENK =   A      = KSO0    = 39
TCK  =   B      = KSO12   = 51
TMS  =   E      = KSO13   = 52
TDI  =   D      = KSO14   = 53
TDO  =   C      = KSO5    = 44




19733-1  header 

A = 13
B = 7
C = 4
D = 22
E = 18


LA- C851P HEADER
A = 7
B = 19
C = 10
D = 21
E = 20

LA-J781P HEADER
A = 20
B = 8
C = 17
D = 6
E = 7
