// Parameters are below for convenience of switching by FFC with different number of contacts.
// [KB_pins =] number of pins for the keyboard connector (24/25/26/28/30/32/34)
// LEFT or RIGHT. If you install the FFC from yourself into the connector, the first contact on the left, then LEFT. In another case, RIGHT.
// UP or DOWN - Contacts in the keyboard connector are at the up or down. 
// 05MM or 08MM or 1MM   contact pitch keyboard connector  

LA-7852P KB_pins=30 LEFT DOWN 1MM KSO3=15 KSI4=4 KSI7=2 KSI6=3 KSI5=6
LA-7912P KB_pins=26 RIGHT UP 1MM KSO3=4 KSI4=23 KSI7=26 KSI6=25 KSI5=24
LA-7981P (JKB1) KB_pins=30 KSO3=18 KSI4=5 KSI7=2 KSI6=3 KSI5=6
LA-7981P (JKB2) KB_pins=24 KSO3=7 KSI4=20 KSI7=23 KSI6=22 KSI5=19
LA-7982P (JKB1) KB_pins=30 KSO3=18 KSI4=5 KSI7=2 KSI6=3 KSI5=6
LA-7982P (JKB2) RIGHT  DOWN  KB_pins=24 KSO3=7 KSI4=20 KSI7=23 KSI6=22 KSI5=19
LA-7983P KB_pins=30 LEFT 1MM KSO3=18 KSI4=5 KSI7=2 KSI6=3 KSI5=6
LA-7988P KSO3=18 KSI4=5 KSI7=2 KSI6=3 KSI5=6


LA-8002P KSO3=13 KSI4=26 KSI7=29 KSI6=28 KSI5=25
LA-8127P KSO3=18 KSI4=5 KSI7=2 KSI6=3 KSI5=6
LA-8131P KSO3=18 KSI4=5 KSI7=2 KSI6=3 KSI5=6
LA-8133P KSO3=18 KSI4=5 KSI7=2 KSI6=3 KSI5=6
LA-8203P KSO3=4 KSI4=23 KSI7=26 KSI6=25 KSI5=24
LA-8221P KB_pins=24 LEFT DOWN KSO3=22 KSI4=15 KSI7=17 KSI6=16 KSI5=19
LA-8222P KB_pins=24 LEFT DOWN KSO3=8 KSI4=9 KSI7=4 KSI6=6 KSI5=7
LA-8223P KB_pins=24 RIGHT UP KSO3=8 KSI4=9 KSI7=4 KSI6=6 KSI5=7
LA-8224P KB_pins=24 LEFT DOWN KSO3=22 KSI4=15 KSI7=17 KSI6=16 KSI5=19
LA-8241P KB_pins=30 LEFT DOWN 08MM KSO3=15 KSI4=4 KSI7=2 KSI6=3 KSI5=6
LA-8262P KSO3=18 KSI4=5 KSI7=2 KSI6=3 KSI5=6
LA-8331P KSO3=4 KSI4=23 KSI7=26 KSI6=25 KSI5=24
LA-8371P KSO3=8 KSI4=9 KSI7=4 KSI6=6 KSI5=7
LA-8391P KSO3=24 KSI4=9 KSI7=12 KSI6=6 KSI5=7
LA-8392P KB_pins=34 LEFT UP 08MM KSO3=24 KSI4=9 KSI7=12 KSI6=6 KSI5=7 KB9012 
LA-8531P KSO3=4 KSI4=23 KSI7=26 KSI6=25 KSI5=24
LA-8611P (JKB1) KSO3=18 KSI4=5 KSI7=2 KSI6=3 KSI5=6
LA-8671P (JKB1) KSO3=18 KSI4=5 KSI7=2 KSI6=3 KSI5=6
LA-8681P (JKB1) KB_pins=30 LEFT DOWN 1MM KSO3=18 KSI4=5 KSI7=2 KSI6=3 KSI5=6 (SS)
LA-8681P (JKB2) KB_pins=24 KSO3=7 KSI4=20 KSI7=23 KSI6=22 KSI5=19
LA-8821P KB_pins=30 KSO3=15 KSI4=4 KSI7=2 KSI6=3 KSI5=6
LA-8861P KB_pins=25 LEFT DOWN 1MM KSO3=22 KSI4=16 KSI7=11 KSI6=12 KSI5=14
LA-8863P KSO3=22 KSI4=16 KSI7=11 KSI6=12 KSI5=14
LA-8864P KSO3=22 KSI4=16 KSI7=11 KSI6=12 KSI5=14
LA-8868P KSO3=22 KSI4=16 KSI7=11 KSI6=12 KSI5=14
LA-8941P KSO3=8 KSI4=14 KSI7=20 KSI6=17 KSI5=16
LA-8943P KSO3=8 KSI4=14 KSI7=20 KSI6=17 KSI5=16
LA-8951P KSO3=9 KSI4=22 KSI7=25 KSI6=24 KSI5=21
LA-8952P KSO3=9 KSI4=22 KSI7=25 KSI6=24 KSI5=21
LA-8971P KB_pins=30 LEFT 1MM KSO3=18 KSI4=5 KSI7=2 KSI6=3 KSI5=6

LA-9001P KSO3=9 KSI4=22 KSI7=25 KSI6=24 KSI5=21
LA-9061P KSO3=13 KSI4=26 KSI7=29 KSI6=28  KSI5=25
LA-9063P KB_pins=30 LEFT 1MM DOWN KSO3=13 KSI4=26 KSI7=29 KSI6=28 KSI5=25
LA-9101P KSO3=16 KSI4=27 KSI7=29 KSI6=28 KSI5=25
LA-9102P KB_pins=30 LEFT DOWN KSO3=16 KSI4=27 KSI7=29 KSI6=28 KSI5=25
LA-9104P KB_pins=30 LEFT DOWN 08MM KSO3=16 KSI4=27 KSI7=29 KSI6=28 KSI5=25
LA-9161P KSO3=26 KSI4=10 KSI7=13 KSI6=7 KSI5=8
LA-9262P KB_pins=30 LEFT DOWN 1MM KSO3=15 KSI4=4 KSI7=2 KSI6=3 KSI5=6 (SS)
LA-9301P SOLDER_ONLY (JECDB2) KSO3=1 KSI4=4 KSI7=3 KSI6=2 KSI5=5      KB_pins=6 
LA-9331P SOLDER_ONLY (JP3)    KSO3=45 KSI4=38 KSI7=41 KSI6=40 KSI5=39 KB_pins=60
LA-9315P KSO3=18 KSI4=5 KSI7=2 KSI6=3 KSI5=6
LA-9531P KB_pins=26 RIGHT UP 1MM KSO3=4 KSI4=23 KSI7=26 KSI6=25 KSI5=24
LA-9532P KSO3=4 KSI4=23 KSI7=26 KSI6=25 KSI5=24
LA-9535P KSO3=4 KSI4=23 KSI7=26 KSI6=25 KSI5=24
LA-9631P KSO3=18 KSI4=5 KSI7=2 KSI6=3 KSI5=6
LA-9632P KB_pins=30 (JKB1) LEFT DOWN 1MM KSO3=18 KSI4=5 KSI7=2 KSI6=3 KSI5=6
LA-9641P KB_pins=30 (JKB1) LEFT DOWN 1MM KSO3=18 KSI4=5 KSI7=2 KSI6=3 KSI5=6
LA-9671P KSO3=13 KSI4=5 KSI7=2 KSI6=3 KSI5=6
LA-9761P KB_pins=32 LEFT DOWN 05MM KSO3=18 KSI4=5 KSI7=2 KSI6=3 KSI5=6

LA-9851P KSO3=18 KSI4=5 KSI7=2 KSI6=3 KSI5=6
LA-9865P KB_pins=34 LEFT UP KSO3=24 KSI4=9 KSI7=12 KSI6=6 KSI5=7
LA-9901P KB_pins=30 (JKB1) LEFT KSO3=18 KSI4=5 KSI7=2 KSI6=3 KSI5=6
LA-9902P KB_pins=30 (JKB1) LEFT KSO3=18 KSI4=5 KSI7=2 KSI6=3 KSI5=6
LA-9911P (JKB1) 1MM LEFT DOWN KSO3=18 KSI4=5 KSI7=2 KSI6=3 KSI5=6
LA-9912P (JKB1) KB_pins=30 1MM LEFT DOWN KSO3=18 KSI4=5 KSI7=2 KSI6=3 KSI5=6
LA-9941P KSO3=15 KSI4=4 KSI7=2 KSI6=3 KSI5=6
LA-9981P KB_pins=30 LEFT DOWN 08MM KSO3=16 KSI4=27 KSI7=29 KSI6=28 KSI5=25
LA-9982P KB_pins=30 LEFT DOWN 08MM KSO3=16 KSI4=27 KSI7=29 KSI6=28 KSI5=25
LA-9984P KSO3=16 KSI4=27 KSI7=29 KSI6=28 KSI5=25

LA-A001P KB_pins=26 RIGHT UP 1MM KSO3=4 KSI4=23 KSI7=26 KSI6=25 KSI5=24
LA-A021P KB_pins=26 RIGHT UP 1MM KSO3=4 KSI4=23 KSI7=26 KSI6=25 KSI5=24
LA-A091P (JKB1) KB_pins=30 LEFT DOWN 1MM KSO3=18 KSI4=5 KSI7=2 KSI6=3 KSI5=6
LA-A092P KSO3=13 KSI4=26 KSI7=29 KSI6=28 KSI5=25
LA-A111P (JECDB1) KSO3=1 KSI4=4 KSI7=3 KSI6=2 KSI5=5
LA-A171P KSO3=18 KSI4=5 KSI7=2 KSI6=3 KSI5=6
LA-A321P KSO3=9 KSI4=22 KSI7=25 KSI6=24 KSI5=21
LA-A341P KSO3=18 KSI4=5 KSI7=2 KSI6=3 KSI5=6
LA-A342P KB_pins=32 LEFT DOWN 05MM KSO3=18 KSI4=5 KSI7=2 KSI6=3 KSI5=6
LA-A481P KSO3=24 KSI4=9 KSI7=12 KSI6=6 KSI5=7
LA-A491P KB_pins=30 LEFT DOWN 08MM KSO3=16 KSI4=27 KSI7=29 KSI6=28 KSI5=25
LA-A521P KB_pins=30 1MM LEFT DOWN KSO3=18 KSI4=5 KSI7=2 KSI6=3 KSI5=6
LA-A551P (JKB4) KB_pins=34                             KSO3=24 KSI4=9 KSI7=12 KSI6=6 KSI5=7
LA-A551P (JKB5) KB_pins=34 LEFT UP 08MM KSO3=24 KSI4=9 KSI7=12 KSI6=6 KSI5=7
LA-A621P KSO3=4 KSI4=23 KSI7=26 KSI6=25 KSI5=24
LA-A681P KSO3=8 KSI4=9 KSI7=4 KSI6=6 KSI5=7
LA-A921P KB_pins=26 LEFT DOWN 08MM KSO3=18 KSI4=5 KSI7=2 KSI6=3 KSI5=6
LA-A961P KSO3=8 KSI4=9 KSI7=4 KSI6=6 KSI5=7
LA-A992P KB_pins=32 LEFT DOWN 1MM KSO3=18 KSI4=5 KSI7=2 KSI6=3 KSI5=6 (SS)
LA-A993P KSO3=18 KSI4=5 KSI7=2 KSI6=3 KSI5=6
LA-A994P KB_pins=32 LEFT DOWN KSO3=18 KSI4=5 KSI7=2 KSI6=3 KSI5=6
LA-A996P KB_pins=32 LEFT DOWN 1MM KSO3=18 KSI4=5 KSI7=2 KSI6=3 KSI5=6
LA-A999P KSO3=18 KSI4=5 KSI7=2 KSI6=3 KSI5=6

LA-B012P KSO3=14 KSI4=4 KSI7=2 KSI6=3 KSI5=6
LA-B015P KSO3=16 KSI4=27 KSI7=29 KSI6=28 KSI5=25
LA-B016P KSO3=16 KSI4=27 KSI7=29 KSI6=28 KSI5=25
LA-B102P KSO3=18 KSI4=5 KSI7=2 KSI6=3 KSI5=6
LA-B111P KB_pins=30 LEFT DOWN 1MM KSO3=18 KSI4=5 KSI7=2 KSI6=3 KSI5=6
LA-B151P KB_pins=28 LEFT DOWN KSO3=7 KSI4=16 KSI7=13 KSI6=24 KSI5=17
LA-B152P KSO3=7 KSI4=16 KSI7=13 KSI6=24 KSI5=17
LA-B161P (JKB1) KB_pins=26 UP RIGHT 1MM KSO3=4 KSI4=23 KSI7=26 KSI6=25 KSI5=24
LA-B162P (JKB1) KB_pins=26 UP RIGHT 1MM KSO3=4 KSI4=23 KSI7=26 KSI6=25 KSI5=24
LA-B211P KSO3=4 KSI4=23 KSI7=26 KSI6=25 KSI5=24
LA-B221P KSO3=4 KSI4=23 KSI7=26 KSI6=25 KSI5=24
LA-B222P KSO3=4 KSI4=23 KSI7=26 KSI6=25 KSI5=24
LA-B231P KSO3=4 KSI4=23 KSI7=26 KSI6=25 KSI5=24
LA-B232P KSO3=4 KSI4=23 KSI7=26 KSI6=25 KSI5=24
LA-B301P_34pin KSO3=24 KSI4=9 KSI7=12 KSI6=6 KSI5=7
LA-B302P_34pin KSO3=24 KSI4=9 KSI7=12 KSI6=6 KSI5=7
LA-B303P_34pin KSO3=24 KSI4=9 KSI7=12 KSI6=6 KSI5=7
LA-B481P KB_pins=30 LEFT DOWN 08MM KSO3=16 KSI4=27 KSI7=29 KSI6=28 KSI5=25
LA-B511P KSO3=4 KSI4=23 KSI7=26 KSI6=25 KSI5=24
LA-B651P KB_pins=30 LEFT DOWN 08MM KSO3=16 KSI4=27 KSI7=29 KSI6=28 KSI5=25
LA-B702P KB_pins=26 UP RIGHT KSO3=4 KSI4=23 KSI7=26 KSI6=25 KSI5=24
LA-B731P KB_pins=26 LEFT UP 08MM   KSO3=23 KSI4=4 KSI7=1 KSI6=2 KSI5=3
LA-B751P KSO3=22 KSI4=21 KSI7=26 KSI6=24 KSI5=23
LA-B753P KSO3=22 KSI4=21 KSI7=26 KSI6=24 KSI5=23
LA-B912P KB_pins=30 LEFT DOWN 08MM KSO3=16 KSI4=27 KSI7=29 KSI6=28 KSI5=25
LA-B972P KSO3=18 KSI4=5 KSI7=2 KSI6=3 KSI5=6
LA-B981P KSO3=4 KSI4=23 KSI7=26 KSI6=25 KSI5=24
LA-B991P KB_pins=26 RIGHT UP 1MM KSO3=4 KSI4=23 KSI7=26 KSI6=25 KSI5=24

LA-C011P KSO3=16 KSI4=27 KSI7=29 KSI6=28 KSI5=25
LA-C021P KSO3=7 KSI4=16 KSI7=13 KSI6=24 KSI5=17
LA-C142P KB_pins=30 LEFT DOWN 08MM KSO3=16 KSI4=27 KSI7=29 KSI6=28 KSI5=25
LA-C341P KB_pins=28 KSO3=23 KSI4=4 KSI7=1 KSI6=2 KSI5=3
LA-C442P KB_pins=34 KSO3=3 KSI4=18 KSI7=15 KSI6=21 KSI5=20
LA-C482P KB_pins=32 KSO3=15 KSI4=28 KSI7=31 KSI6=30 KSI5=27
LA-C502P KB_pins=32 LEFT DOWN 1MM KSO3=15 KSI4=28 KSI7=31 KSI6=30 KSI5=27
LA-C503P KB_pins=32 KSO3=15 KSI4=28 KSI7=31 KSI6=30 KSI5=27
LA-C571P KB_pins=30 LEFT DOWN 08MM KSO3=16 KSI4=27 KSI7=29 KSI6=28 KSI5=25
LA-C701P KB_pins=32 LEFT DOWN 1MM KSO3=18 KSI4=5 KSI7=2 KSI6=3 KSI5=6
LA-C781P KSO3=18 KSI4=5 KSI7=2 KSI6=3 KSI5=6
LA-C801P KB_pins=28 LEFT UP KSO3=23 KSI4=4 KSI7=1 KSI6=2 KSI5=3
LA-C811P KB_pins=32 LEFT DOWN 1MM KSO3=18 KSI4=5 KSI7=2 KSI6=3 KSI5=6
LA-C912P KSO3=22 KSI4=21 KSI7=26 KSI6=24 KSI5=23
LA-C921P KSO3=18 KSI4=5 KSI7=2 KSI6=3 KSI5=6
LA-C991P KSO3=15 KSI4=28 KSI7=31 KSI6=30 KSI5=27

LA-D121P KB_pins=26 RIGHT UP 1MM KSO3=4 KSI4=23 KSI7=26 KSI6=25 KSI5=24
LA-D591P KSO3=23 KSI4=6 KSI7=3 KSI6=4 KSI5=5
LA-D641P KB_pins=28 LEFT UP 1MM KSO3=23 KSI4=4 KSI7=1 KSI6=2 KSI5=3
LA-D661P KB_pins=28 LEFT UP 1MM KSO3=23 KSI4=4 KSI7=1 KSI6=2 KSI5=3
LA-D671P KB_pins=28 UP LEFT KSO3=23 KSI4=4 KSI7=1 KSI6=2 KSI5=3
LA-D702P KB_pins=32 LEFT DOWN 1MM KSO3=18 KSI4=5 KSI7=2 KSI6=3 KSI5=6
LA-D703P KB_pins=32 LEFT DOWN 1MM KSO3=18 KSI4=5 KSI7=2 KSI6=3 KSI5=6
LA-D704P KSO3=18 KSI4=5 KSI7=2 KSI6=3 KSI5=6
LA-D707P KSO3=18 KSI4=5 KSI7=2 KSI6=3 KSI5=6
LA-D711P KSO3=18 KSI4=5 KSI7=2 KSI6=3 KSI5=6
LA-D713P KSO3=18 KSI4=5 KSI7=2 KSI6=3 KSI5=6
LA-D751P (JEC) KB_pins=8 KSO3=1 KSI4=4 KSI5=5 KSI7=3 KSI6=2 
LA-D753P (JEC) KB_pins=8 KSO3=1 KSI4=4 KSI5=5 KSI7=3 KSI6=2 
LA-D803P KB_pins=30 LEFT DOWN 08MM KSO3=16 KSI4=27 KSI7=29 KSI6=28 KSI5=25
LA-D804P KB_pins=30 LEFT DOWN 08MM KSO3=16 KSI4=27 KSI7=29 KSI6=28 KSI5=25

LA-D921P KSO3=23 KSI4=4 KSI7=1 KSI6=2 KSI5=3

LA-E061P KB_pins=28 UP LEFT KSO3=23 KSI4=4 KSI7=1 KSI6=2 KSI5=3
LA-E361P (JKB1) KB_pins=32 RIGHT UP 1MM KSO3=10 KSI4=29 KSI7=32 KSI6=31 KSI5=30
LA-E791P KSO3=15 KSI4=28 KSI7=31 KSI6=30 KSI5=27
LA-E801P KB_pins=32 LEFT DOWN 1MM KSO3=15 KSI4=28 KSI7=31 KSI6=30 KSI5=27
LA-E811P KB_pins=32 LEFT DOWN 1MM KSO3=15 KSI4=28 KSI7=31 KSI6=30 KSI5=27
LA-E831P KB_pins=32 LEFT DOWN 1MM KSO3=15 KSI4=28 KSI7=31 KSI6=30 KSI5=27
LA-E841P KB_pins=32 LEFT DOWN 1MM KSO3=15 KSI4=28 KSI7=31 KSI6=30 KSI5=27
LA-E892P (JKB1) KB_pins=28 UP LEFT 1MM KSO3=23 KSI4=4 KSI7=1 KSI6=2 KSI5=3
LA-E903P KB_pins=28 LEFT UP 1MM KSO3=23 KSI4=4 KSI7=1 KSI6=2 KSI5=3
LA-E911P (JKB1) KB_pins=32 RIGHT UP 1MM KSO3=10 KSI4=29 KSI7=32 KSI6=31 KSI5=30
LA-E911P (JKB2) KB_pins=28 LEFT UP 1MM KSO3=23 KSI4=4 KSI7=1 KSI6=2 KSI5=3

LA-E921P (JKB1) KB_pins=32 RIGHT UP 1MM KSO3=10 KSI4=29 KSI7=32 KSI6=31 KSI5=30 (SS)
LA-E921P (JKB2) KB_pins=28 LEFT         KSO3=23 KSI4=4 KSI7=1 KSI6=2 KSI5=3 (SS)

LA-F013P KB_pins=32 RIGHT DOWN 05MM KSO3=18 KSI4=5 KSI7=2 KSI6=3 KSI5=6 (Milan Leposavic)
LA-F031P KB_pins=32 LEFT DOWN 1MM KSO3=15 KSI4=28 KSI7=31 KSI6=30 KSI5=27
LA-F121P KSO3=16 KSI4=27 KSI7=29 KSI6=28 KSI5=25
LA-F421p KB_pins=32 LEFT DOWN 05MM KSO3=14 KSI4=5 KSI7=2 KSI6=3 KSI5=12
LA-F483P KB_pins=32 LEFT DOWN 08MM KSO3=9 KSI4=22 KSI7=25 KSI6=24 KSI5=21
LA-F486P KB_pins=32 LEFT DOWN 08MM KSO3=9 KSI4=22 KSI7=25 KSI6=24 KSI5=21
LA-F661P KB_pins=32 LEFT DOWN 08MM KSO3=24 KSI4=11 KSI7=8 KSI6=9 KSI5=12 KB9022 (Desjet)
LA-F761P KB_pins=32 LEFT DOWN 1MM KSO3=15 KSI4=28 KSI7=31 KSI6=30 KSI5=27
LA-F841P (JKB1) KB_pins=32 LEFT DOWN 1MM KSO3=15 KSI4=28 KSI7=31 KSI6=30 KSI5=27
LA-F861P (JKB1) KB_pins=32 LEFT DOWN 1MM KSO3=15 KSI4=28 KSI7=31 KSI6=30 KSI5=27
LA-F943P (JKB1) KB_pins=28 LEFT UP 1MM KSO3=23 KSI4=4 KSI7=1 KSI6=2 KSI5=3
LA-F951P KB_pins=28 LEFT UP 1MM KSO3=23 KSI4=4 KSI7=1 KSI6=2 KSI5=3
LA-F952P KB_pins=28 LEFT UP 1MM KSO3=23 KSI4=4 KSI7=1 KSI6=2 KSI5=3
LA-F991P (JKB1) KB_pins=32 RIGHT UP 1MM KSO3=10 KSI4=29 KSI7=32 KSI6=31 KSI5=30
 
LA-G202P KSO3=9  KSI4=22 KSI7=25 KSI6=24 KSI5=21
LA-G021P (JKB2) KB_pins=28 1MM LEFT UP KSO3=23 KSI4=4 KSI7=1 KSI6=2 KSI5=3  KB9022Q
LA-G078P KB_pins=32 1MM DOWN LEFT KSO3=15 KSI4=28 KSI7=31 KSI6=30 KSI5=27   KB9022Q
LA-G07EP KB_pins=32 1MM DOWN LEFT KSO3=15 KSI4=28 KSI7=31 KSI6=30 KSI5=27
LA-G07FP KB_pins=32 1MM DOWN LEFT KSO3=15 KSI4=28 KSI7=31 KSI6=30 KSI5=27   KB9022Q
LA-G07CP KB_pins=32 1MM DOWN LEFT KSO3=13 KSI4=28 KSI7=31 KSI6=30 KSI5=27 KB9022Q
LA-G07DP KB_pins=32 1MM DOWN LEFT KSO3=15 KSI4=28 KSI7=31 KSI6=30 KSI5=27 KB9022Q
LA-G07JP KB_pins=32 1MM DOWN LEFT KSO3=15 KSI4=28 KSI7=31 KSI6=30 KSI5=27 KB9022Q
LA-G073P KB_pins=32 1MM DOWN LEFT KSO3=15 KSI4=28 KSI7=31 KSI6=30 KSI5=27 KB9022Q
LA-G076P KB_pins=32 1MM DOWN LEFT KSO3=15 KSI4=28 KSI7=31 KSI6=30 KSI5=27
LA-G081P                          KSO3=7 KSI4=16 KSI7=13 KSI6=24 KSI5=17 (semmi32)
LA-G094P KB_pins=30 RIGHT DOWN 08MM KSO3=15 KSI4=4 KSI7=2 KSI6=3 KSI5=6
LA-G131P KB_pins=10 LEFT DOWN 05MM FLASH=160 KSO3=2 KSI4=9 KSI7=6 KSI6=7 KSI5=8  KB9542Q
LA-G241P KB_pins=32 08MM LEFT DOWN KSO3=9 KSI4=22 KSI7=25 KSI6=24 KSI5=21 KB9022Q
LA-G521P KB_pins=28 LEFT UP 1MM KSO3=23 KSI4=6 KSI7=3 KSI6=4 KSI5=5 KB9022Q
LA-G541P (JKB1) KB_pins=32 KSO3=24 KSI4=11 KSI7=8 KSI6=9 KSI5=12 KB9022Q
LA-G581P KB_pins=32 RIGHT DOWN 08MM KSO3=9 KSI4=22 KSI7=25 KSI6=24 KSI5=21 KB9022Q

LA-H082P KB_pins=32 LEFT DOWN 08MM KSO3=24 KSI4=11 KSI7=8 KSI6=9 KSI5=12
LA-H091P KB_pins=32 LEFT DOWN 08MM KSO3=20 KSI4=11 KSI7=8 KSI6=9 KSI5=12 
LA-H101P KB_pins=32 RIGHT UP 08MM KSO3=9 KSI4=22 KSI7=25 KSI6=24 KSI5=21
LA-H103P KSO3=24 KSI4=11 KSI7=8 KSI6=9 KSI5=12
LA-H104P KB_pins=32 RIGHT UP 08MM KSO3=9 KSI4=22 KSI7=25 KSI6=24 KSI5=21 
LA-H105P KB_pins=32 LEFT UP 08MM KSO3=24 KSI4=11 KSI7=8 KSI6=9 KSI5=12
LA-H131P KB_pins=32 LEFT UP 08MM KSO3=24 KSI4=11 KSI7=8 KSI6=9 KSI5=12 kb9022q 
LA-H323P KB_pins=32 1MM DOWN LEFT KSO3=15 KSI4=28 KSI7=31 KSI6=30 KSI5=27 KB9022Q 
LA-H431P KB_pins=28 LEFT UP 1MM KSO3=23 KSI4=6 KSI7=3 KSI6=4 KSI5=5 KB9022Q
LA-H462P KB_pins=32 1MM DOWN LEFT FLASH=160 KSO3=15 KSI4=28 KSI7=31 KSI6=30 KSI5=27 
LA-H463P KB_pins=32 1MM DOWN LEFT FLASH=160 KSO3=15 KSI4=28 KSI7=31 KSI6=30 KSI5=27 KB9542Q 
LA-H472P KB_pins=32 1MM DOWN LEFT KSO3=15 KSI4=28 KSI7=31 KSI6=30 KSI5=27 KB9022Q 
LA-H501P KB_pins=28 LEFT UP 1MM KSO3=23 KSI4=6 KSI7=3 KSI6=4 KSI5=5 KB9022Q (LEX66)
LA-H781P KB_pins=28 LEFT UP 1MM KSO3=23 KSI4=6 KSI7=3 KSI6=4 KSI5=5 KB9022Q (77romantik77)
LA-H782P KB_pins=28 LEFT UP 1MM KSO3=23 KSI4=6 KSI7=3 KSI6=4 KSI5=5 KB9022Q (stsaper)
LA-H792P KB_pins=28 LEFT UP 1MM KSO3=23 KSI4=6 KSI7=3 KSI6=4 KSI5=5 KB9022Q (stsaper)
LA-H801P KB_pins=28 LEFT UP 1MM KSO3=23 KSI4=6 KSI7=3 KSI6=4 KSI5=5 KB9022Q

LA-K181P KB_pins=28 LEFT UP 1MM KSO3=23 KSI4=6 KSI7=3 KSI6=4 KSI5=5 KB9022Q (Ciber SLasH)
LA-K201P KB_pins=32 1MM  KSO3=15 KSI4=28 KSI7=31 KSI6=30 KSI5=27 KB9052Q

LA-J151P KB_pins=28 LEFT UP 1MM    KSO3=23 KSI4=6 KSI7=3 KSI6=4 KSI5=5 KB9022Q (Serge_L)
LA-J551P KB_pins=34 LEFT DOWN 08MM KSO3=9 KSI4=22 KSI7=25 KSI6=24 KSI5=21 KB9052Q (Marvell)
LA-J561P KB_pins=6  LEFT DOWN 05MM KSO3=5 KSI4=1 KSI5=2 KSI6=3 KSI7=4 FLASH=160 KB9542Q (bushmann)
LA-J701P KB_pins=34 LEFT DOWN 08MM KSO3=9 KSI4=22 KSI7=25 KSI6=24 KSI5=21 KB9022Q (Desjet)
LA-J731P KB_pins=28 LEFT UP 08MM   KSO3=22 KSI4=4 KSI7=1 KSI6=2 KSI5=3 KB9022Q
LA-J801P KB_pins=28 LEFT UP 1MM    KSO3=23 KSI4=6 KSI7=3 KSI6=4 KSI5=5 KB9052Q (SS)
LA-J861P KB_pins=28 LEFT UP 1MM    KSO3=23 KSI4=6 KSI7=3 KSI6=4 KSI5=5 

LA-L171  KB_pins=12 KSO3=0 KSI4=4 KSI7=1 KSI6=2 KSI5=3 (12pins Debug port) KB9022

LA-L181  KB_pins=32 KSO3=23 KSI4=6 KSI7=3 KSI6=4 KSI5=5


NM-A044 KB_pins=32 RIGHT DOWN 05MM KSO3=15 KSI4=28 KSI7=31 KSI6=30 KSI5=27

DAG54AMB6D0 KB_pins=32 LEFT 1MM DOWN KSO3=15 KSI4=28 KSI7=31 KSI6=30 KSI5=27  KB9027Q
DAG55AMB6E0 KB_pins=32 LEFT 1MM DOWN KSO3=15 KSI4=28 KSI7=31 KSI6=30 KSI5=27  KB9027Q
DA00P2MB6D0 KSO3=15 KSI4=28 KSI7=31 KSI6=30 KSI5=27
DA0X21MB6D0 KSO3=15 KSI4=28 KSI7=31 KSI6=30 KSI5=27
DA0X22MB6D0 KSO3=15 KSI4=28 KSI7=31 KSI6=30 KSI5=27
DA0U82MB6D0  KB_pins=32  LEFT 1MM DOWN KSO3=15 KSI4=28 KSI7=31 KSI6=30 KSI5=27
DA0U83MB6E0 KB_pins=32 (CN5) 1MM LEFT DOWN KSO3=15 KSI4=28 KSI7=31 KSI6=30 KSI5=27
DA0Y08MBAD0 KSO3=18 KSI4=5 KSI7=2 KSI6=3 KSI5=6
DAY22AMB6F0  KB_pins=32 LEFT DOWN 1MM KSO3=15 KSI4=28 KSI7=31 KSI6=30 KSI5=27
DAY23AMB6F0  KSO3=15 KSI4=28 KSI7=31 KSI6=30 KSI5=27
DA0Y72MB6C0 KB_pins=32 LEFT 1MM DOWN KSO3=18 KSI4=5 KSI7=2 KSI6=3 KSI5=6

CHEWBACCA_14_WHL_UMA KB_pins=32 LEFT DOWN 1MM KSO3=15 KSI4=28 KSI7=31 KSI6=30 KSI5=27 KB9028Q (ksandr13)
Kroyer/Yeats      KB_pins=32 LEFT DOWN 1MM KSO3=15 KSI4=28 KSI7=31 KSI6=30 KSI5=27    
FAROE_1.0_GML     KB_pins=32 LEFT DOWN 1MM KSO3=15 KSI4=28 KSI7=31 KSI6=30 KSI5=27 KB9028Q (merlin)
Fauchon-SKY       KB_pins=32 LEFT DOWN 1MM KSO3=15 KSI4=28 KSI7=31 KSI6=30 KSI5=27    
Lakers_U42_MB     KB_pins=32 LEFT DOWN 1MM KSO3=15 KSI4=28 KSI7=31 KSI6=30 KSI5=27 KB9028G
LEIA_15_KBL_UMA   KB_pins=32 LEFT DOWN 1MM KSO3=15 KSI4=28 KSI7=31 KSI6=30 KSI5=27
Bucks_NVDIS       KB_pins=32 LEFT DOWN 1MM KSO3=15 KSI4=28 KSI7=31 KSI6=30 KSI5=27  KB9028
Bucks_UMA         KB_pins=32 LEFT DOWN 1MM KSO3=15 KSI4=28 KSI7=31 KSI6=30 KSI5=27  KB9028
BUZZ              KB_pins=28 LEFT UP       KSO3=23 KSI4=6 KSI7=3 KSI6=4 KSI5=5
Brittle           KB_pins=32 LEFT DOWN 1MM KSO3=15 KSI4=28 KSI7=31 KSI6=30 KSI5=27 (LEX66)
Brook_BH          KB_pins=28 UP LEFT 1MM   KSO3=23 KSI4=4 KSI7=1 KSI6=2 KSI5=3
Gale_4G           KB_pins=32 LEFT DOWN 1MM KSO3=15 KSI4=28 KSI7=31 KSI6=30 KSI5=27 KB9028G
GHIBLI 18803      KB_pins=28               KSO3=23 KSI4=6 KSI7=3 KSI6=4 KSI5=5 KB9028Q
Goya/Balen        KB_pins=32 LEFT DOWN     KSO3=18 KSI4=5 KSI7=2 KSI6=3 KSI5=6
Katniss           KB_pins=30 LEFT DOWN 1MM KSO3=18 KSI4=5 KSI7=2 KSI6=3 KSI5=6 KB9028G (kalya)
Rayleigh-SL                                KSO3=23 KSI4=4 KSI7=1 KSI6=2 KSI5=3 KB9028
NBA_Laker         KB_pins=32 LEFT DOWN 1MM KSO3=15 KSI4=28 KSI7=31 KSI6=30 KSI5=27 KB9028G 
NBA_Rockets_MB    KB_pins=32 LEFT DOWN 1MM KSO3=15 KSI4=28 KSI7=31 KSI6=30 KSI5=27 KB9028G
NFL_SR_17         KB_pins=32               KSO3=15 KSI4=28 KSI7=31 KSI6=30 KSI5=27 KB9028Q (Zhuk)
Nougat-BSW                                 KSO3=7 KSI4=16 KSI7=13 KSI6=24 KSI5=17
Newgate_SLS DDR5  KB_pins=28 LEFT UP 1MM   KSO3=23 KSI4=4 KSI7=1 KSI6=2 KSI5=3
Mihawk 15208-2    KB_pins=24 UP RIGHT 1MM  KSO3=17 KSI4=11 KSI7=5 KSI6=8 KSI5=9
Pikachu_WHL       KB_pins=28 LEFT UP 1MM   KSO3=23 KSI4=6 KSI7=3 KSI6=4 KSI5=5 KB9028Q (HyperFreq)
AMD_PICASSO       KB_pins=30 LEFT DOWN 08MM KSO3=27 KSI4=10 KSI7=7 KSI6=8 KSI5=9 KB9028Q (Денис Скляров)
WOODY_KBL_R       KB_pins=28 LEFT UP       KSO3=23 KSI4=6 KSI7=3 KSI6=4 KSI5=5
SLINKY            KB_pins=28 LEFT UP 1MM   KSO3=23 KSI4=6 KSI7=3 KSI6=4 KSI5=5 KB9028Q
Strongbow         KB_pins=28 RIGHT 1MM     KSO3=23 KSI4=6 KSI7=3 KSI6=4 KSI5=5 KB9028Q 
Hevin-BSW	  KB_pins=28 LEFT DOWN 1MM KSO3=7  KSI4=16 KSI7=13 KSI6=24 KSI5=17 KB9028Q
Sapporo_GLK_MB    KB_pins=28 LEFT UP       KSO3=23 KSI4=6 KSI7=3 KSI6=4 KSI5=5 KB9028Q
NP530U3B LOTUS13-R KB_pins=25  RIGHT KSO3=4 KSI4=10 KSI7=15 KSI6=14 KSI5=12       
NP535U4C LOTUS14-CML KB_pins=25  RIGHT KSO3=4 KSI4=10 KSI7=15 KSI6=14 KSI5=12  
NP900X3B AMOR2-13 KB_pins=30 DOWN 1MM RIGHT KSO3=4 KSI4=10 KSI7=15 KSI6=14 KSI5=12
NP550P5C MCLAREN KB_pins=25 RIGHT DOWN 1MM KSO3=4 KSI4=10 KSI7=15 KSI6=14 KSI5=12
NP550P5C MCLAREN KSO3=22 KSI4=16 KSI7=11 KSI6=12 KSI5=14 (первый ближе к АКБ и прямой шлейф 24  1в1)


ASUS E402SA KB_pins=24 LEFT DOWN 1MM KSO3=8 KSI4=9 KSI7=4 KSI6=6 KSI5=7
ASUS E406MA KB_pins=30 LEFT DOWN 08MM KSO3=9 KSI4=16 KSI7=14 KSI6=15 KSI5=12 KB902AQ
ASUS K501LX KB_pins=24 1MM KSO3=8 KSI4=9 KSI7=4 KSI6=6 KSI5=7 
ASUS X302LA KB_pins=24 LEFT DOWN 1MM KSO3=17 KSI4=16 KSI7=21 KSI6=19 KSI5=18
ASUS X405UA KB_pins=30 LEFT DOWN 08MM KSO3=22 KSI4=15 KSI7=17 KSI6=16 KSI5=19 KB9026
ASUS X455LJ KB_pins=24 LEFT  1MM  KSO3=8 KSI4=9 KSI7=4 KSI6=6 KSI5=7
ASUS X540SA KB_pins=26 08MM KSO3=8 KSI4=9 KSI7=4 KSI6=6 KSI5=7
ASUS X540MA KB_pins=26 08MM LEFT DOWN KSO3=8 KSI4=9 KSI7=4 KSI6=6 KSI5=7 (elixirby)
ASUS X540MB KB_pins=26 08MM LEFT DOWN KSO3=8 KSI4=9 KSI7=4 KSI6=6 KSI5=7
ASUS X540NA KB_pins=26 08MM LEFT DOWN KSO3=8 KSI4=9 KSI7=4 KSI6=6 KSI5=7
ASUS X540NV KB_pins=26 08MM LEFT DOWN KSO3=8 KSI4=9 KSI7=4 KSI6=6 KSI5=7
ASUS X540UP KB_pins=26 08MM LEFT DOWN KSO3=8 KSI4=9 KSI7=4 KSI6=6 KSI5=7
ASUS X540SC KB_pins=26 08MM LEFT DOWN KSO3=8 KSI4=9 KSI7=4 KSI6=6 KSI5=7
ASUS X541NA KB_pins=26 08MM LEFT DOWN KSO3=8 KSI4=9 KSI7=4 KSI6=6 KSI5=7
ASUS X541NС KB_pins=26 08MM LEFT DOWN KSO3=8 KSI4=9 KSI7=4 KSI6=6 KSI5=7
ASUS X756UA KB_pins=24 LEFT DOWN 1MM KSO3=17 KSI4=16 KSI7=21 KSI6=19 KSI5=18
ASUS X756UV KB_pins=24 LEFT DOWN 1MM KSO3=8 KSI4=9 KSI7=4 KSI6=6 KSI5=7
ASUS X756UX KB_pins=24 LEFT DOWN 1MM KSO3=8 KSI4=9 KSI7=4 KSI6=6 KSI5=7

MS-14A11 KB_pins=26 LEFT DOWN 1MM KSO3=4 KSI4=21 KSI7=24 KSI6=23 KSI5=22 KB9028Q (Евгений18)
MS-16K21 KB_pins=26 LEFT 1MM KSO3=4 KSI4=13 KSI7=16 KSI6=15 KSI5=14 
MS-16P11 KB_pins=30 RIGHT UP 05MM KSO3=27 KSI4=18 KSI7=15 KSI6=16 KSI5=17
MS-16P51 KB_pins=26 LEFT UP 1MM KSO3=23 KSI4=14 KSI7=11 KSI6=12 KSI5=13 KB9028Q
MS-16P61 KB_pins=26 LEFT    1MM KSO3=4 KSI4=13 KSI7=16 KSI6=15 KSI5=14
MS-16P71 KB_pins=26 LEFT UP 1MM KSO3=23 KSI4=14 KSI7=11 KSI6=12 KSI5=13 KB9028Q
MS-16R11 KB_pins=30 RIGHT UP 05MM KSO3=27 KSI4=18 KSI7=15 KSI6=16 KSI5=17 (SS)
MS-16R31 KB_pins=30 LEFT  UP 05MM KSO3=4 KSI4=13 KSI7=16 KSI6=15 KSI5=14 KB9028Q  (kulibinnik)
MS-16R41 KB_pins=30 RIGHT UP 05MM KSO3=27 KSI4=18 KSI7=15 KSI6=16 KSI5=17 (Rimas)
MS-16U41 KB_pins=26 LEFT UP 1MM KSO3=23 KSI4=14 KSI7=11 KSI6=12 KSI5=13 (i-wind)
MS-16J41 KB_pins=26 LEFT 1MM UP KSO3=23 KSI4=14 KSI7=11 KSI6=12 KSI5=13  kb9028q
MS-16J51 KB_pins=26 LEFT UP 1MM KSO3=23 KSI4=14 KSI7=11 KSI6=12 KSI5=13 (dobry)
MS-16J61 KB_pins=26 LEFT UP 1MM KSO3=23 KSI4=14 KSI7=11 KSI6=12 KSI5=13   kb9028q
MS-16J91 KB_pins=26 LEFT UP 1MM KSO3=23 KSI4=14 KSI7=11 KSI6=12 KSI5=13 (within1915)
MS-16JB1                        KSO3=23 KSI4=14 KSI7=11 KSI6=12 KSI5=13 
MS-16JF1 KB_pins=26 LEFT UP 1MM KSO3=23 KSI4=14 KSI7=11 KSI6=12 KSI5=13 kb9028q (VaultDweller)
MS-16W11 KB_pins=30 RIGHT UP 05MM KSO3=27 KSI4=18 KSI7=15 KSI6=16 KSI5=17 KB9028Q (smoke)
MS-16Q21 KB_pins=30 LEFT DOWN 05MM KSO3=4 KSI4=13 KSI7=16 KSI6=15 KSI5=14
MS-17A11 KB_pins=26 KSO3=4 KSI4=13 KSI7=16 KSI6=15 KSI5=14 LEFT 1MM
MS-17F11 KB_pins=26 KSO3=23 KSI4=14 KSI7=11 KSI6=12 KSI5=13 KB9028Q (Андрей Загорский)
MS-17F41 KB_pins=26 LEFT UP 1MM    KSO3=23 KSI4=14 KSI7=11 KSI6=12 KSI5=13 KB9028Q
MS-17F61 KB_pins=26 KSO3=23 KSI4=14 KSI7=11 KSI6=12 KSI5=13 KB9028Q (bass)
MS-17821            KSO3=4 KSI4=13 KSI7=16 KSI6=15 KSI5=14
MS-17831 KB_pins=26 KSO3=4 KSI4=13 KSI7=16 KSI6=15 KSI5=14 LEFT 1MM
MS-17851 KB_pins=26 KSO3=4 KSI4=13 KSI7=16 KSI6=15 KSI5=14 LEFT 1MM
MS-18121 KB_pins=26 LEFT DOWN 1MM KSO3=4 KSI4=13 KSI7=16 KSI6=15 KSI5=14 (Igor GaRR)
MicroXperts HSW131-T (MB NPB VER C)    KSO3=18 KSI4=9 KSI7=12 KSI6=1 KSI5=8
Diner: KSO3=18 KSI4=5 KSI7=2 KSI6=3 KSI5=6
Franky_CZ MB 14278-2 KSO3=23 KSI4=4 KSI7=1 KSI6=2 KSI5=3
DOMINO BH 15300-1 MB KSO3=4 KSI4=23 KSI7=26 KSI6=25 KSI5=24
Panini BSW KB_pins=32 DOWN RIGHT 1MM KSO3=18 KSI4=5 KSI7=2 KSI6=3 KSI5=6   KB9029Q ?? 
OPP 17 Diner SKL_KBL UMA_DIS 15289-2 448.08E01.0021  KSO3=15 KSI4=28 KSI7=31 KSI6=30 KSI5=27 KB9028Q
Laduree1.0 MB 14257-2 KB_pins=32 LEFT DOWN 1MM KSO3=15 KSI4=28 KSI7=31 KSI6=30 KSI5=27
Hevin-Sky KSO3=7 KSI4=16 KSI7=13 KSI6=24 KSI5=17
NE116WB2_V10 KB_pins=26 1MM KSO3=18 KSI4=5 KSI7=2 KSI6=3 KSI5=6

120S-11&14IAP (J5502)  KB_pins=32 LEFT DOWN 08MM KSO3=9  KSI4=22 KSI7=25 KSI6=24 KSI5=21 KB9028Q
320s-13                KB_pins=32 DOWN LEFT 08MM KSO3=9  KSI4=22 KSI7=25 KSI6=24 KSI5=21
330s_kbl_mb_v06        KB_pins=32 UP   LEFT 08MM KSO3=24 KSI4=11 KSI7=1  KSI6=9  KSI5=12
330s_kbl_mb_v09        KB_pins=32 UP   LEFT 08MM KSO3=24 KSI4=11 KSI7=1  KSI6=9  KSI5=12
330s_ast_mb_v10        KB_pins=32 UP   LEFT 08MM KSO3=26 KSI4=11 KSI7=1  KSI6=9  KSI5=12 KB9028Q (SS) 
yoga330_mb_v06         KB_pins=32 UP   LEFT 08MM KSO3=9  KSI4=23 KSI7=25 KSI6=24 KSI5=21 KB9028Q (veseliy) 

1501B_01_01 (CONI1) KB_pins=26 LEFT DOWN 1MM KSO3=18 KSI4=5 KSI7=2 KSI6=3 KSI5=6 KB9028Q

CORVO_15_MB 18741 KB_pins=32 KSO3=15 KSI4=28 KSI7=31 KSI6=30 KSI5=27 KB9028Q
KNICKS 16280-2    KB_pins=28 LEFT DOWN 1MM KSO3=7  KSI4=16 KSI7=13 KSI6=24 KSI5=17 KB9028Q
17893-1   KB_pins=28 LEFT UP 1MM   KSO3=23 KSI4=6 KSI7=3 KSI6=4 KSI5=5 KB9028Q