USER MANUAL


**Introduction**

The FT232HL is a USB-to-serial interface chip designed and manufactured by FTDI (Future Technology Devices International). It provides a simple and flexible way to interface microcontrollers and other devices with a USB port, and it can also be used as an SPI (Serial Peripheral Interface) or I2C (Inter-Integrated Circuit) programmer. This manual will guide you through the setup and use of the FT232HL chip for programming devices over SPI or I2C.

**Key Features:**

* Laptop SPI I2C Bios Chip Read Write Operations
* USB to SPI/I2C communication support
* 1.8V 3.3V and 5V Support
* Simple interface for embedded system communication
* Flexible control for custom applications
* High data transfer rate up to 12 Mbps for SPI and I2C

**MARUTI BIOS PROGRAMMER EXPLAIN**



**MARUTI Laptop SPI I2C BIOS Chip Read and Write Operations – Installation and Software Guide**

Thank you for choosing the MARUTI BIOS Programmer. This guide provides step-by-step instructions for setting up and using the software to read and write BIOS chips effectively.

**Driver Installation**

1. **Plug-and-Play Ready:**  
   No additional driver installation is required. The device utilizes a default virtual driver that is already installed on your system.

**Steps for Reading and Writing BIOS Chips**

1. **Insert the BIOS Chip:**  
   Place the BIOS chip securely in the SPI slot of the MARUTI programmer.
2. **Select Voltage:**  
   Set the appropriate voltage on the programmer switch based on your BIOS chip specifications:
   * 1.8V
   * 3.3V
   * 5.0V
3. **Launch the Software:**  
   Open the MARUTI BIOS Programmer software on your computer.
4. **Detect the Chip:**
   * Click on the “Detect BIOS Chip” option in the software.
   * The software will scan and identify the chip.
5. **Select the Chip:**
   * From the detected list, select the specific chip model you want to operate on.
6. **Read the Chip:**
   * Click the “Read Chip” button to read the data stored in the chip.
   * Wait for the process to complete.
7. **Save the Read File:**
   * After reading, save the BIOS file to a desired location on your computer for backup or reference.
8. **Open a New BIOS File:**
   * If you wish to update the chip, open the new BIOS file you want to write.
   * Use the “Open” option in the software to load the file.
9. **Write to the Chip:**
   * Click on the “Write + Unprotect + Verify” option to start writing the new BIOS data to the chip.
   * The software will automatically unprotect the chip, write the new data, and verify the write process.
10. **Completion:**
    * Once the write process is successfully completed, the operation is done.
    * You may now remove the chip from the programmer.

**Important Notes:**

* Ensure the BIOS chip is properly seated in the SPI slot to avoid any errors during the process.
* Always save the original BIOS file before making any changes for recovery purposes.
* If any issues occur, refer to the troubleshooting section of the user manual or contact MARUTI support.

### ****Other Uses of FT232HL-Based MARUTI BIOS Programmer****

Apart from its primary functionality of reading and writing SPI and I2C BIOS chips, the MARUTI BIOS Programmer has several additional applications that make it a versatile tool for various fields. Here are some other uses explained:

### ****1. Debugging SPI/I2C Protocols****

* The programmer can act as a **protocol analyzer** to debug SPI or I2C communication between devices.
* It allows monitoring and troubleshooting data transmission in embedded systems, such as microcontrollers or sensors.

### ****2. Embedded Systems Development****

* **Firmware Development:**  
  Useful for uploading, testing, and debugging firmware on EEPROM, microcontrollers, or other embedded devices.
* **Bootloader Programming:**  
  It supports programming bootloaders for microcontroller-based systems, allowing you to initialize and customize systems easily.

### ****3. EEPROM Programming****

* The EEPROM interface is designed to program various types of EEPROM chips.
* Useful for recovering or cloning firmware stored in EEPROMs used in devices such as:
  + Home appliances
  + Medical equipment
  + Industrial systems

### ****4. Laptop and Motherboard Repair****

* A valuable tool for technicians performing repairs on laptops or motherboards by enabling:
  + Backup of BIOS/UEFI firmware.
  + Restoration of corrupted firmware.
  + Updating outdated firmware to support new hardware.

### ****5. Reverse Engineering****

* It is ideal for reverse engineering SPI/I2C devices by:
  + Reading and analyzing firmware or configuration data.
  + Modifying chip content to understand proprietary systems.

### ****6. Chip Cloning****

* Enables cloning of SPI or I2C BIOS chips or EEPROMs by:
  + Reading data from a functioning chip.
  + Writing the same data to a blank or damaged chip for replacement purposes.

### ****7. Hobbyist Projects****

* **IoT Development:**  
  Use it to interface with SPI/I2C-based IoT devices, such as temperature sensors, displays, and more.
* **DIY Electronics:**  
  Ideal for programming custom devices or chips for hobbyist projects.

### ****8. Education and Training****

* Excellent for teaching and learning SPI and I2C communication protocols in academic or training settings.
* Demonstrates practical applications of BIOS programming and embedded systems.

### ****9. Data Recovery****

* **Firmware Recovery:**  
  Recover lost or corrupted firmware data from damaged BIOS chips or EEPROMs.
* **Configuration Backup:**  
  Backup and restore critical configuration files stored in memory chips.

### ****10. General Voltage Source****

* Provides a stable **1.8V**, **3.3V**, or **5.0V** power source for testing circuits and peripherals, making it useful for:
  + Debugging electronics.
  + Powering small embedded systems.

### ****11. Development of Custom Devices****

* You can interface the programmer with custom-built devices for development and testing purposes, such as:
  + Creating custom IoT devices.
  + Experimenting with SPI/I2C devices in advanced prototyping scenarios.

### ****12. Automotive Applications****

* Used in the automotive industry for:
  + Reprogramming ECUs (Engine Control Units) with SPI/I2C-based firmware.
  + Backing up or modifying firmware in automotive embedded systems.

### ****13. Serial Communication Interface****

* Can be used as a general-purpose USB-to-SPI/I2C interface for controlling or monitoring devices in real time.

### ****Why Choose the MARUTI BIOS Programmer for These Applications?****

* **Wide Compatibility:** Supports various voltages and protocols.
* **Ease of Use:** Plug-and-play operation with intuitive software.
* **Versatility:** Multi-purpose tool for multiple industries, including IT, automotive, and education.
* **Compact Design:** Portable and easy to integrate into a technician’s toolkit.

Let me know if you'd like detailed explanations for specific use cases or guidance on implementing these functions!

