
ITE not detected reason  (busy id error) 
1. ITE pin 58 to 63 all pins must be have between the 2.8v to 3.3v (check this before connect the programmer) 
2. use original adapter instead of power supply or extension pin 
3. fcc cable is faulty 
4. wrong selected fcc cable (0.8mm , 1 mm  pitch) 
5. Do not give a power while you click step 2 but connect power before click on step 3 in software 
6. always share connection photos programmer to motherboard along with software clear screenshot 
7. wrong database configuration


ITE pin 58 to 63 all pins 
isko check kijiye KB CONN SE BEEP KR RHA HAI

Lost communication error occurred due to the following reason  
1. fcc cable faulty  
2. use a short-length USB cable 
3. use the original adapter  
4. check the USB ground cable  
5. ENE faulty or motherboard fault  
6. check pin numbers 33 and 37 pins of the io controller while you were getting this error