[INFO] Connecting to COM3

[<-TX] Handshake request (COM3)
3D 00 02 01 00 03

[RX->] Handshake response
3D 00 08 81 00 53 42 48 41 43 4B 35

[INFO] Handshake OK: SBHACK

[INFO] Device connected (COM3)

[RX->] Device settings
3D 00 05 83 01 03 00 00 8C

[INFO] Word byte-order: reverse read/write

[INFO] Design voltage: 0.0 V

[<-TX] Scan SMBus
3D 00 02 02 02 06

[RX->] Scan SMBus address result
3D 00 03 82 02 FF 86

[INFO] No SMBus device found

[<-TX] Scan SMBus
3D 00 02 02 02 06

[RX->] Scan SMBus address result
3D 00 03 82 02 FF 86

[INFO] No SMBus device found

[<-TX] Scan SMBus
3D 00 02 02 02 06

[RX->] Scan SMBus address result
3D 00 03 82 02 FF 86

[INFO] No SMBus device found

[<-TX] Scan SMBus
3D 00 02 02 02 06

[RX->] Scan SMBus address result
3D 00 03 82 02 FF 86

[INFO] No SMBus device found

[<-TX] Scan SMBus
3D 00 02 02 02 06

[RX->] Scan SMBus address result
3D 00 03 82 02 FF 86

[INFO] No SMBus device found

[<-TX] Scan SMBus
3D 00 02 02 02 06

[RX->] Scan SMBus address result
3D 00 03 82 02 FF 86

[INFO] No SMBus device found

[<-TX] Scan SMBus
3D 00 02 02 02 06

[RX->] Scan SMBus address result
3D 00 03 82 02 FF 86

[INFO] No SMBus device found

[RX->] Device is ready
3D 00 03 80 01 00 84

[<-TX] Scan SMBus
3D 00 02 02 02 06

[RX->] Scan SMBus address result
3D 00 03 82 02 FF 86

[INFO] No SMBus device found

[<-TX] Scan SMBus
3D 00 02 02 02 06

[RX->] Scan SMBus address result
3D 00 03 82 02 FF 86

[INFO] No SMBus device found

[<-TX] Scan SMBus
3D 00 02 02 02 06

[RX->] Scan SMBus address result
3D 00 03 82 02 0B 92

[INFO] SMBus device(s): 0B

[<-TX] Scan SMBus
3D 00 02 02 02 06

[RX->] Scan SMBus address result
3D 00 03 82 02 0B 92

[INFO] SMBus device(s): 0B

[<-TX] SMBus register dump request
3D 00 04 02 03 00 27 30

[RX->] SMBus register dump (00-27)
3D 00 7C 82 03 00 27 00 00 00 01 01 18 02 00 0A 03 60 01 04 00 00 05 FF FF 06 FF FF 07 00 01 08 
0B DF 09 3A 0B 0A 00 00 0B 00 00 0C 00 01 0D 00 00 0E 00 00 0F 00 00 10 06 1D 11 FF FF 12 FF FF 
13 FF FF 14 07 A8 15 43 30 16 02 D0 17 03 D3 18 0A F0 19 39 D0 1A 00 31 1B 44 37 1C 19 F2 1D 19 
F2 1E 19 F2 1F 19 F2 20 31 05 21 4F 07 22 4C 04 23 50 02 24 50 02 25 50 02 26 50 02 27 50 02 1D

[INFO] SMBus register dump details (00-27):
[00]: 00 00 // ManufacturerAccess: 00 00
[01]: 01 18 // RemainingCapacityAlarm: 280 mAh
[02]: 00 0A // RemainingTimeAlarm: 10 minutes
[03]: 60 01 // BatteryMode: 0110000000000001
[04]: 00 00 // AtRate: 0 minutes
[05]: FF FF // AtRateTimeToFull: 65535 minutes
[06]: FF FF // AtRateTimeToEmpty: 65535 minutes
[07]: 00 01 // AtRateOK: true
[08]: 0B DF // Temperature: 27.66°C
[09]: 3A 0B // Voltage: 14.859 V
[0A]: 00 00 // Current: 0 A
[0B]: 00 00 // AverageCurrent: 0 A
[0C]: 00 01 // MaxError: 1%
[0D]: 00 00 // RelativeStateOfCharge: 0%
[0E]: 00 00 // AbsoluteStateOfCharge: 0%
[0F]: 00 00 // RemainingCapacity: 0 mAh
[10]: 06 1D // FullChargeCapacity: 1565 mAh
[11]: FF FF // RunTimeToEmpty: 65535 minutes
[12]: FF FF // AverageTimeToEmpty: 65535 minutes
[13]: FF FF // AverageTimeToFull: 65535 minutes
[14]: 07 A8 // ChargingCurrent: 1.96 A
[15]: 43 30 // ChargingVoltage: 17.2 V
[16]: 02 D0 // BatteryStatus: 0000001011010000
[17]: 03 D3 // CycleCount: 979
[18]: 0A F0 // DesignCapacity: 2800 mAh
[19]: 39 D0 // DesignVoltage: 14.8 V
[1A]: 00 31 // SpecificationInfo: 0000000000110001
[1B]: 44 37 // ManufactureDate: 2014.01.23
[1C]: 19 F2 // SerialNumber: 19 F2
[1D]: 19 F2 // 19 F2
[1E]: 19 F2 // 19 F2
[1F]: 19 F2 // 19 F2
[20]: 31 05 // ManufacturerName: 31 05
[21]: 4F 07 // DeviceName: 4F 07
[22]: 4C 04 // DeviceChemistry: 4C 04
[23]: 50 02 // ManufacturerData: 50 02
[24]: 50 02 // 50 02
[25]: 50 02 // 50 02
[26]: 50 02 // 50 02
[27]: 50 02 // 50 02

[<-TX] Scan SMBus
3D 00 02 02 02 06